(footprint "Converter_DCDC_CUI_VX7805-500" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0 -6.35 unlocked) (layer "F.SilkS")
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    (tstamp aec9cf35-a256-4e38-b0fa-b40dbdf2443b)
  )
  (fp_text value "Converter_DCDC_CUI_VX7805-500" (at 0 3.8 unlocked) (layer "F.Fab")
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    (tstamp cfba1af9-c945-469a-81c0-89a4fe0bee83)
  )
  (fp_text user "${REFERENCE}" (at 0 5.25 unlocked) (layer "F.Fab")
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    (tstamp fc9278fa-7c71-48e0-a7cd-46dd879bd676)
  )
  (fp_rect (start -5.8 -5.38) (end 5.8 2.13)
    (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp 115ca6bf-f6c5-4678-8559-31c76cdafa2a))
  (fp_circle (center -4.35 2.625) (end -3.85 2.625)
    (stroke (width 0.12) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 32c4558c-5fef-46af-9824-44fdf0f0f69a))
  (fp_rect (start -6.05 -5.625) (end 6.05 2.375)
    (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp 94e1aebe-a34e-4509-89bd-e64d65731424))
  (pad "1" thru_hole roundrect (at -2.54 0) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25) (tstamp 7503e1c1-b6db-42d2-b36e-093fda7e47a3))
  (pad "2" thru_hole circle (at 0 0) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask") (tstamp c1710706-e6df-4c25-873b-f50566bb13b8))
  (pad "3" thru_hole circle (at 2.54 0) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask") (tstamp ed5bd2d8-38f2-4fa1-a93c-ea543dc48178))
  (model "${KIPRJMOD}/../assets/3dmodels/VX7805-500.stp"
    (offset (xyz 0 1.25 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
