(footprint "R_0603_HandSolder" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0 -1.2 unlocked) (layer "F.SilkS") hide
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    (tstamp 65821dc9-86d3-40d3-8fb1-f7f960a457a7)
  )
  (fp_text value "R_0603_HandSolder" (at 0 1.275 unlocked) (layer "F.Fab") hide
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    (tstamp 2a1ea671-1d32-4f21-b558-4b1bf8716412)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
    (tstamp 5fe24b8a-1e96-4739-bf47-63398f989256)
  )
  (fp_line (start -0.35 0.2) (end -0.25 -0.2)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 88690416-95a1-46d3-a579-dd694327c49b))
  (fp_line (start -0.25 -0.2) (end -0.15 0.2)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4e297da1-a109-42f7-9880-d42edbe6de71))
  (fp_line (start -0.15 0.2) (end -0.05 -0.2)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 13e7ae99-1f72-4549-9fdf-8b5f9c5437b1))
  (fp_line (start -0.05 -0.2) (end 0.05 0.2)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2a3d2d49-a25b-4164-ae87-90443341570d))
  (fp_line (start 0.05 0.2) (end 0.15 -0.2)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp bb008b97-8665-4a2e-8749-73fea04a284b))
  (fp_line (start 0.15 -0.2) (end 0.25 0.2)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 85aa8476-914e-4ffa-9f14-58d3e0a65223))
  (fp_line (start 0.25 0.2) (end 0.35 -0.2)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 220b47f9-712e-45e4-b01e-184334b1524d))
  (fp_rect (start -1.6 -0.6) (end 1.6 0.6)
    (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp fea6b512-ea6f-437e-8a96-c6ae04bdcf6b))
  (fp_line (start -1.65 -0.73) (end 1.65 -0.73)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3a6a8fc8-8f20-43eb-b851-78b4fdd072a2))
  (fp_line (start -1.65 0.73) (end -1.65 -0.73)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b3fd8a19-f2f1-45cc-8e01-fa3f633d848f))
  (fp_line (start 1.65 -0.73) (end 1.65 0.73)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0b1c9365-2dc4-40e0-9d91-165b9bea37ae))
  (fp_line (start 1.65 0.73) (end -1.65 0.73)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp afee8df8-ab01-4e16-942c-f8818b4d32af))
  (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9f74bf8d-cccb-40f6-9dfb-3442d08a2ef0))
  (fp_line (start -0.8 0.4125) (end -0.8 -0.4125)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp cca47f69-0c0c-46f7-95d3-9938fa1bef53))
  (fp_line (start 0.8 -0.4125) (end 0.8 0.4125)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c6bba2e4-e595-4d0c-9575-2be8b2271a9e))
  (fp_line (start 0.8 0.4125) (end -0.8 0.4125)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 95a4e1d9-523e-43b4-bbd6-15454f0e80d4))
  (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 6780ca72-1b58-4175-8d56-c0503dd7b3c3))
  (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 45ccb97d-4413-4a47-83e0-53fef2e6515e))
  (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
