(footprint "JST_X_B3B-XH-AM_1x03_P2.50mm_Vertical" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 3 -3.45 unlocked) (layer "F.SilkS")
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    (tstamp 8723df2a-9ab6-48cc-b001-f2720949f261)
  )
  (fp_text value "JST_X_B3B-XH-AM_1x03_P2.50mm_Vertical" (at 2.5 4.55 unlocked) (layer "F.Fab")
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    (tstamp a77d4539-4842-4c9f-b576-b055af4ff3df)
  )
  (fp_text user "${REFERENCE}" (at 2.55 2.7) (layer "F.Fab")
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    (tstamp 23cf86c7-381b-4d33-b096-f846a6b5bece)
  )
  (fp_line (start -2.8 -2.75) (end -2.8 -1.5)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f066505a-170d-4a62-9dcb-17e0a7fd4662))
  (fp_line (start -2.51 -2.46) (end -2.51 3.51)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 85b6a346-1f01-4f01-88fb-e2c6a05d81e6))
  (fp_line (start -2.51 3.51) (end 7.61 3.51)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a065d6ec-28de-4532-959e-edb440ee62af))
  (fp_line (start -2.5 -2.45) (end -2.5 -1.7)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9ea7ac93-cd7d-4bd1-aa1b-f77fc2e0e8c0))
  (fp_line (start -2.5 -1.7) (end -0.7 -1.7)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 59e9e929-7e0a-4e02-b986-b51118e4ec0e))
  (fp_line (start -2.5 -0.2) (end -1.75 -0.2)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 05c87da3-34a6-49a3-b456-167f760ee91c))
  (fp_line (start -1.75 -0.2) (end -1.75 1.14)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ddde7ed5-7aa6-4c76-a41b-37ddf2633013))
  (fp_line (start -1.55 -2.75) (end -2.8 -2.75)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f04341ed-61dc-4534-af23-3fe02444ac79))
  (fp_line (start -0.7 -2.45) (end -2.5 -2.45)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 323f91e6-bc14-4150-ae6a-86dc298ece6a))
  (fp_line (start -0.7 -1.7) (end -0.7 -2.45)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a3698a22-8716-4118-9b4e-a265d05f93e7))
  (fp_line (start 0.8 -2.45) (end 0.8 -1.7)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 490841ac-e730-40df-a598-51801c47a9aa))
  (fp_line (start 0.8 -1.7) (end 4.3 -1.7)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5707f914-ca94-4f98-a41a-bcb3bddfaa36))
  (fp_line (start 2.55 2.75) (end -0.69 2.75)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c9649c66-e2ce-4885-8efe-a266b7a8f81c))
  (fp_line (start 4.3 -2.45) (end 0.8 -2.45)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 96684572-569f-4cd2-978b-b0c6ed733c0f))
  (fp_line (start 4.3 -1.7) (end 4.3 -2.45)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a299dc45-a279-4a86-8f6f-34910b3d2af1))
  (fp_line (start 5.8 -2.45) (end 5.8 -1.7)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4d7ab760-5a04-43b7-b196-d31eaa8d3c21))
  (fp_line (start 5.8 -1.7) (end 7.6 -1.7)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d1f1964b-fda5-4c92-981c-e4e3aa6b5f0e))
  (fp_line (start 6.85 -0.2) (end 6.85 2.75)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7fdcfd0f-fc77-4293-933c-ca9aee11977a))
  (fp_line (start 6.85 2.75) (end 2.55 2.75)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 07ab2d6e-7aa5-40f3-a261-8486dbbfd7fc))
  (fp_line (start 7.6 -2.45) (end 5.8 -2.45)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8bfd03bc-e4df-4bdf-b422-fa9c018912a0))
  (fp_line (start 7.6 -1.7) (end 7.6 -2.45)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 919506e5-217e-4846-bb2a-b5e2e84851ac))
  (fp_line (start 7.6 -0.2) (end 6.85 -0.2)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ce6b58da-7b85-4fc4-b12d-a654029a6b06))
  (fp_line (start 7.61 -2.46) (end -2.51 -2.46)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 369f22a1-e999-4fb9-9ea5-8eba7dfc9c6a))
  (fp_line (start 7.61 3.51) (end 7.61 -2.46)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e8a831f9-b52b-405c-bbf3-0a581b019b10))
  (fp_circle (center 0.05 -1.7) (end 0.65 -1.7)
    (stroke (width 0.12) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 6481a6cf-ef10-4f09-8f93-07a3eb3b33b7))
  (fp_line (start -2.9 -2.85) (end -2.9 3.9)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 7a4c4d44-2957-4c29-8d90-93791883f0bb))
  (fp_line (start -2.9 3.9) (end 8 3.9)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 1cd39ed6-876c-43a5-a04e-2fbbebb863c6))
  (fp_line (start 8 -2.85) (end -2.9 -2.85)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f60455fd-efc8-40f6-a532-e843f27ce4fd))
  (fp_line (start 8 3.9) (end 8 -2.85)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 49c00ac4-f504-4ffe-8aa8-3f7f3715ba75))
  (fp_line (start -2.4 -2.35) (end -2.4 3.4)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f9ecd1fc-571a-4ef0-91ae-f83e7efe0854))
  (fp_line (start -2.4 3.4) (end 7.5 3.4)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 873df387-4598-463f-9aec-0702f2e84d50))
  (fp_line (start -0.575 -2.35) (end 0.05 -1.35)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 935e3885-54a4-46c1-af61-0bd91f994efd))
  (fp_line (start 0.05 -1.35) (end 0.675 -2.35)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1eb16548-bac9-46fe-9b6e-174d396f2fc1))
  (fp_line (start 7.5 -2.35) (end -2.4 -2.35)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b799017d-9b7a-414d-ae6e-d392068cfd74))
  (fp_line (start 7.5 3.4) (end 7.5 -2.35)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c5446bfc-3e6e-4fe8-8902-0ecfedc196ee))
  (pad "" np_thru_hole circle (at -1.55 2) (size 1.2 1.2) (drill 1.2) (layers "*.Cu" "*.Mask") (tstamp 73328e43-3bec-4078-bc22-6627d112337f))
  (pad "1" thru_hole roundrect (at 0.05 0) (size 1.7 1.95) (drill 0.95) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.147059) (tstamp 647ffda6-5bc2-4e20-8de4-a8520a0176e8))
  (pad "2" thru_hole oval (at 2.55 0) (size 1.7 1.95) (drill 0.95) (layers "*.Cu" "*.Mask") (tstamp da33604b-d11e-479c-88ac-4b451d24e253))
  (pad "3" thru_hole oval (at 5.05 0) (size 1.7 1.95) (drill 0.95) (layers "*.Cu" "*.Mask") (tstamp b3ffa22d-48ef-4e73-ad7b-e93dc50ffa98))
  (model "${KIPRJMOD}/../assets/3dmodels/JST_B3B_XH_A.step"
    (offset (xyz 2.55 -0.5 -1))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 -180))
  )
)
