(footprint "D_SOD-323" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0 -1.5 unlocked) (layer "F.SilkS")
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    (tstamp 596572ae-6ceb-466f-a6ba-68720f51a9df)
  )
  (fp_text value "D_SOD-323" (at 0 1.6 unlocked) (layer "F.Fab")
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    (tstamp 1dd30be4-4008-4d67-abe9-6fb3ef05ee81)
  )
  (fp_text user "${REFERENCE}" (at 0 2.65 unlocked) (layer "F.Fab")
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    (tstamp 3590f18b-636d-4c5d-ab2d-c7e1d0bfa18c)
  )
  (fp_line (start -2.45 -0.8) (end 2.2 -0.8)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp b99f83be-8b1a-4317-9d2f-856ce817e782))
  (fp_line (start -0.3 -0.35) (end -0.3 0.35)
    (stroke (width 0.1) (type solid)) (layer "F.SilkS") (tstamp 7caecf09-f3d7-435a-802a-d7b38ff3f679))
  (fp_line (start -0.25 0) (end -0.45 0)
    (stroke (width 0.1) (type solid)) (layer "F.SilkS") (tstamp cdecd73e-fbd4-4c97-9dc6-8a521e8d6f49))
  (fp_line (start 0.25 0) (end 0.45 0)
    (stroke (width 0.1) (type solid)) (layer "F.SilkS") (tstamp 00a23a67-3d3f-436b-9bc1-bf4a9d04f876))
  (fp_line (start 2.2 -0.8) (end 2.2 0.8)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 8aecaf4c-0245-4428-a4c0-ad4372b9dba4))
  (fp_line (start 2.2 0.8) (end -2.45 0.8)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 452e7afa-becc-48ed-9284-de2bb3c486bb))
  (fp_rect (start -2.45 -0.8) (end -2.2 0.8)
    (stroke (width 0.12) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 3f5d983b-9bad-4702-9e5e-43a59992dff6))
  (fp_poly
    (pts
      (xy 0.3 0.4)
      (xy -0.3 0)
      (xy 0.3 -0.4)
    )

    (stroke (width 0.12) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 0938f9d2-5bcb-4b35-9945-8488f4cb51d3))
  (fp_rect (start -2.575 -1) (end 2.425 1)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp d5c876dd-874c-42a7-8cf7-2df6e20ebe67))
  (fp_rect (start -0.8 -0.7) (end 0.8 0.7)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp 8261b9dc-3152-456c-a122-f1810d03fad9))
  (pad "1" smd rect (at -1.45 0) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp bc5d2269-d4f0-4a64-bf1c-bd5f9eab35e8))
  (pad "2" smd rect (at 1.45 0) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp f45022be-b213-4f74-9e09-cc51bbfacaf9))
  (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
