(footprint "C_0402_HandSolder" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0 -1.05 unlocked) (layer "F.SilkS")
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    (tstamp 0edc9b03-018e-4945-885f-32a277e67ae0)
  )
  (fp_text value "C_0402_HandSolder" (at 0 1.2 unlocked) (layer "F.Fab")
      (effects (font (size 0.7 0.7) (thickness 0.15) bold))
    (tstamp d4a73c5e-ef78-4cfc-a496-cd97ad50c502)
  )
  (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.04)))
    (tstamp a1cade20-df26-461f-8e0b-6a4f674a357e)
  )
  (fp_line (start -1 -0.5) (end 1 -0.5)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp c2450ea9-c0d1-4521-8952-f6d8b49b61e8))
  (fp_line (start -1 0.5) (end -1 -0.5)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 2d74a3fa-3e0c-4d57-831d-5aafdcc8b8ed))
  (fp_line (start -0.1 -0.2) (end -0.1 0.2)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b6f89cfb-8e61-49b9-be3c-8da1d3d56aa8))
  (fp_line (start 0.1 0.2) (end 0.1 -0.2)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d7bca089-896e-4773-a351-c8219a1535ab))
  (fp_line (start 1 -0.5) (end 1 0.5)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp bc9f11ee-af40-4841-9152-4ca9a8a5f973))
  (fp_line (start 1 0.5) (end -1 0.5)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 73d9e2cd-2823-4742-8d7c-2d50368bee4d))
  (fp_line (start -1.075 -0.575) (end 1.075 -0.575)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp f785682f-bbd8-4988-97af-3509b2d8b4c1))
  (fp_line (start -1.075 0.575) (end -1.075 -0.575)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 17e69412-8cf3-482d-ab09-68fe2566fee7))
  (fp_line (start 1.075 -0.575) (end 1.075 0.575)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 27372af1-ff60-48be-a18c-3d7e7445281f))
  (fp_line (start 1.075 0.575) (end -1.075 0.575)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 85e66ce2-d055-41fa-a06a-910842832b78))
  (pad "1" smd roundrect (at -0.55 0) (size 0.735 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp bccc1162-760e-4b5d-9ad4-f1fc74dfeb6f))
  (pad "2" smd roundrect (at 0.55 0) (size 0.735 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 74298477-c045-474d-b073-f403c9546d2c))
  (model "${KICAD7_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
