(footprint "JST_SH_SM04B-SRSS" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0 -3.9 unlocked) (layer "F.SilkS")
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    (tstamp a3212ff3-73ba-4c11-9fb7-9ab4e7ea9272)
  )
  (fp_text value "JST_SH_SM04B-SRSS" (at 0 4.1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp f8fb9151-bdad-4656-ae51-f9b5d5238a36)
  )
  (fp_text user "${REFERENCE}" (at 0 -0.03) (layer "F.Fab")
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    (tstamp f7ff64ca-1646-45c3-9c48-f5ea499cd04d)
  )
  (fp_line (start -3.11 -1.815) (end -2.06 -1.815)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 463b9c81-06c0-404d-97f3-d524e7c357eb))
  (fp_line (start -3.11 0.685) (end -3.11 -1.815)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a67e0744-86d7-4fe4-8d5c-843f2a5af8d9))
  (fp_line (start -2.06 -1.815) (end -2.06 -2.805)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 32508a3c-d17d-41a1-85bd-966a7ec54045))
  (fp_line (start -1.94 2.655) (end 1.94 2.655)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3f73008b-4bcd-4e6f-94be-0b5ea5b921bf))
  (fp_line (start 3.11 -1.815) (end 2.06 -1.815)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ec781c72-fdac-4794-b299-1cd951280837))
  (fp_line (start 3.11 0.685) (end 3.11 -1.815)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d97ae555-41df-4792-9cca-8e4898c2e70b))
  (fp_circle (center -2.7 -2.48) (end -2.2 -2.48)
    (stroke (width 0.12) (type solid)) (fill solid) (layer "F.SilkS") (tstamp d4ba0530-5af8-4d87-b9bb-1f204f7e5ae8))
  (fp_line (start -3.9 -3.31) (end -3.9 3.25)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 2e214735-113f-4199-8b2f-611efbc9fb5f))
  (fp_line (start -3.9 3.25) (end 3.9 3.25)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e9a1a8af-a208-4ff4-9ef9-553e183e7e1b))
  (fp_line (start 3.9 -3.31) (end -3.9 -3.31)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ce967d20-d256-480f-a0dd-34209caf6f99))
  (fp_line (start 3.9 3.25) (end 3.9 -3.31)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 99e78206-00f5-49af-b115-c78aa252272f))
  (fp_line (start -3 -1.705) (end -3 2.545)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 769dec41-1262-4891-a972-5a0a264173ea))
  (fp_line (start -3 -1.705) (end 3 -1.705)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 53608e5f-d1ff-4fa2-ab68-33d9f69b1395))
  (fp_line (start -3 2.545) (end 3 2.545)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 73a2b3a3-e0e8-42d4-a662-8d51df2c6afe))
  (fp_line (start -2 -1.705) (end -1.5 -0.997893)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 02e4b36e-0ceb-48ea-a91a-0eca5eb4bf7d))
  (fp_line (start -1.5 -0.997893) (end -1 -1.705)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp cbdb26ea-14a9-419d-9f49-5d70ec59e2da))
  (fp_line (start 3 -1.705) (end 3 2.545)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3e7945b2-55b9-46f7-8d21-77c1ea19ab75))
  (pad "1" smd roundrect (at -1.5 -2.03) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 8cbdbd9e-72de-4756-ba52-0c0107c33e39))
  (pad "2" smd roundrect (at -0.5 -2.03) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp b0b61511-96fb-44ff-9df7-fd003016603c))
  (pad "3" smd roundrect (at 0.5 -2.03) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 18d62617-7bd2-4a0f-8ba6-ee7ce99fa58d))
  (pad "4" smd roundrect (at 1.5 -2.03) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp dac05563-6614-44d0-8d5c-5df40126b72f))
  (pad "MP" smd roundrect (at -2.8 1.845) (size 1.2 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333) (tstamp 9e474343-aae4-476d-8423-3117e3df64e1))
  (pad "MP" smd roundrect (at 2.8 1.845) (size 1.2 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333) (tstamp 755556d4-7c82-46a8-b509-ece789264c84))
  (model "${KIPRJMOD}/../assets/3dmodels/SM04-SRSS-TB.STEP"
    (offset (xyz 0 1.5 -0.4))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
