(footprint "M_N20"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -3.6 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "b7e45296-b75a-41f3-9ede-79b6ced70a7d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "M_N20"
		(at 0 3.7 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "2c52d4c5-8323-4aa3-ae79-f5ed8b1b361f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "d8b33584-56a4-407a-8274-ecd7558c0500")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "9a2f0237-3065-419a-9036-db630be477cb")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "357091f5-04af-422a-90e7-8d711805c475")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_circle
		(center 0 0)
		(end 2.7 0)
		(stroke
			(width 0.2)
			(type default)
		)
		(fill none)
		(layer "Edge.Cuts")
		(uuid "e4d4096f-693b-477e-8186-40fa7d73c800")
	)
	(fp_line
		(start -3.301514 4.95)
		(end 3.301513 4.95)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "F.Fab")
		(uuid "985db59a-330d-466d-b265-12ef1c01d004")
	)
	(fp_line
		(start -3.301514 4.95)
		(end 3.301515 4.95)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "F.Fab")
		(uuid "eea97083-118f-4b87-8418-116bd396840d")
	)
	(fp_line
		(start 3.301513 -4.95)
		(end -3.301514 -4.95)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "F.Fab")
		(uuid "e7a1241b-26db-4b7b-b41c-5640a5899ce2")
	)
	(fp_line
		(start 3.301513 -4.95)
		(end -3.301514 -4.95)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "F.Fab")
		(uuid "f9c344d0-bc2c-486a-8132-3eca9114e9fd")
	)
	(fp_arc
		(start -3.301514 4.95)
		(mid -5.95 0)
		(end -3.301514 -4.95)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "F.Fab")
		(uuid "1fe763d4-01b1-47ea-8ed6-e7e01b47a2ce")
	)
	(fp_arc
		(start -3.301514 4.95)
		(mid -5.95 0)
		(end -3.301514 -4.95)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "F.Fab")
		(uuid "c8073ea9-8a24-4d35-86a7-be9aedf4e058")
	)
	(fp_arc
		(start 3.301513 -4.95)
		(mid 5.949999 0)
		(end 3.301513 4.95)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "F.Fab")
		(uuid "826a4b44-e857-406a-9ac8-22781eca003d")
	)
	(fp_arc
		(start 3.301513 -4.95)
		(mid 5.949999 0)
		(end 3.301513 4.95)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "F.Fab")
		(uuid "d43b1223-8054-44a0-8c6b-629cc25072b4")
	)
	(fp_circle
		(center 0 0)
		(end 2.5 0)
		(stroke
			(width 0.2)
			(type default)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "9a54703c-a987-433b-8775-48399a79487d")
	)
	(fp_circle
		(center 0 0)
		(end 2.5 0)
		(stroke
			(width 0.2)
			(type default)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "e37ff277-4fb4-454c-8748-915c1db4f52c")
	)
	(fp_text user "${REFERENCE}"
		(at 0 5.8 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "674653fa-53e3-4fd1-9f18-7d790c29f550")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole oval
		(at -3.55 0)
		(size 1.15 3)
		(drill oval 0.9 2.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "ecd69b4d-5992-415f-831a-35c3d9be3894")
	)
	(pad "2" thru_hole oval
		(at 3.55 0)
		(size 1.15 3)
		(drill oval 0.9 2.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "c6914aa6-705b-4a7c-aba5-1d01fe44b87a")
	)
	(model "/home/cynt4k-emgenics/Documents/Privat/pcb-droid/hardware/pcbs/assets/3dmodels/n20-motor.step"
		(offset
			(xyz 0 0 -1.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 90 0 0)
		)
	)
)
