(footprint "USB_C_Receptacle_JAE_DX07S016JA1R1500" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "USB TYPE C, USB 2.0, SMT, https://www.jae.com/en/connectors/series/detail/product/id=91780")
  (tags "USB C Type-C Receptacle SMD USB 2.0")
  (property "Sheetfile" "connections.kicad_sch")
  (property "Sheetname" "Connections")
  (property "ki_description" "USB 2.0-only Type-C Receptacle connector")
  (property "ki_keywords" "usb universal serial bus type-C USB2.0")
  (property "mpn" "DX07S016JA1R1500")
  (attr smd)
  (fp_text reference "J407" (at 0 -5 -180) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 371865a1-2494-4c80-a5fd-ea34ca798d82)
  )
  (fp_text value "DX07S016JA1R1500" (at 0 5 -180) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 9a6485b6-12a8-40e0-b0a6-47c1b3852ce9)
  )
  (fp_text user "${REFERENCE}" (at 0 0 -180) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp a4c2a1d4-641f-4b4a-a439-0ab746e91730)
  )
  (fp_line (start -4.58 -1.215) (end -4.58 -0.36)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9e649d6c-dbd4-45cc-a221-1890bc3f382c))
  (fp_line (start -4.58 2.76) (end -4.58 3.71)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8f7b9e28-6ed1-4e09-a91b-56204f18b964))
  (fp_line (start -4.58 3.71) (end 4.58 3.71)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0c4c6fce-754c-4045-bb1c-323d367644c7))
  (fp_line (start 4.58 -1.215) (end 4.58 -0.36)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ff42525e-8156-424a-bd93-247e0e72b686))
  (fp_line (start 4.58 2.76) (end 4.58 3.71)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c5a4222e-b636-4b94-ae2c-83a7a702d367))
  (fp_line (start -5.47 -4.33) (end -5.47 4.1)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b274b63b-9771-4d80-ba28-73833c096baa))
  (fp_line (start -5.47 -4.33) (end 5.47 -4.33)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 985ae714-45df-4fbe-85dc-936c617d64f1))
  (fp_line (start -5.47 4.1) (end 5.47 4.1)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 52324638-6cf1-4cc1-b33a-694ebb880fd1))
  (fp_line (start 5.47 -4.33) (end 5.47 4.1)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 704e5459-04df-4f65-89c8-f7423877ce47))
  (fp_line (start -4.47 -3.3) (end -4.47 3.6)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 94ba7229-9703-41ba-8c25-71cd0447d92e))
  (fp_line (start -4.47 -3.3) (end 4.47 -3.3)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b0fe6629-bd51-4ac2-a917-24e67b586758))
  (fp_line (start -4.47 3.6) (end 4.47 3.6)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 663b3807-1f7e-4044-abfb-568dbadfa921))
  (fp_line (start 4.47 -3.3) (end 4.47 3.6)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 141da4a7-b588-4a31-9675-6aec4ca39191))
  (pad "" np_thru_hole circle (at -3 -1.95) (size 0.6 0.6) (drill 0.6) (layers "F&B.Cu" "*.Mask") (tstamp 64a7fdbe-f8a1-4fbe-b146-ffd6ac7d1f34))
  (pad "" smd rect (at -1.4 1.15) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp b148b2bc-6c2c-424a-b1f0-e5147b2686db))
  (pad "" smd rect (at 1.4 1.15) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 6d3397e5-db5c-4331-9b9f-3b6e55cadc6f))
  (pad "" np_thru_hole oval (at 3 -1.95) (size 0.85 0.6) (drill oval 0.85 0.6) (layers "F&B.Cu" "*.Mask") (tstamp 6ab1dfb9-f06a-41fe-b6c4-0df257b093a6))
  (pad "A1" smd rect (at -3.1 -3.05) (size 0.52 1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 29c6afc7-1240-4556-bb05-28520dba4967))
  (pad "A4" smd rect (at -2.35 -3.05) (size 0.52 1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 646b01f0-4f2e-4267-b9af-95e6645052d6))
  (pad "A5" smd rect (at -1.75 -3.05) (size 0.27 1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 11c243ad-1c96-44fb-8ae4-89a920d35d76))
  (pad "A6" smd rect (at -0.25 -3.05) (size 0.27 1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 4bfb9356-949f-4298-8036-4018320e6446))
  (pad "A7" smd rect (at 0.75 -3.05) (size 0.27 1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 92d40ac1-671e-4771-9126-88983d9626f4))
  (pad "A8" smd rect (at 1.75 -3.05) (size 0.27 1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp bba345bc-0b3a-46b3-9a75-3e6f9f4d4712))
  (pad "A9" smd rect (at 2.35 -3.05) (size 0.52 1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 8ea7cb5c-2ed6-4030-91a9-ad5246caec9e))
  (pad "A12" smd rect (at 3.1 -3.05) (size 0.52 1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 9f0f6510-4c4b-49cd-9439-03dc83cd0968))
  (pad "B1" smd rect (at 3.1 -3.05) (size 0.52 1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 336d655d-765d-4b28-a46d-734f450aba17))
  (pad "B4" smd rect (at 2.35 -3.05) (size 0.52 1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 1be2bdce-0a86-41e4-a543-41e219a30aed))
  (pad "B5" smd rect (at 1.25 -3.05) (size 0.27 1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 702c0620-145d-42d6-8bb5-ec52d983bd9e))
  (pad "B6" smd rect (at 0.25 -3.05) (size 0.27 1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 81c754de-3d98-4513-a6f4-bc088fe6ab3a))
  (pad "B7" smd rect (at -0.75 -3.05) (size 0.27 1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 31f104ab-b0db-4ce7-b11d-8d46e880c827))
  (pad "B8" smd rect (at -1.25 -3.05) (size 0.27 1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 2ee1c4a2-ce3e-40c0-8dfb-f48e9704accd))
  (pad "B9" smd rect (at -2.35 -3.05) (size 0.52 1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 690df968-3a4b-475a-8403-157977240598))
  (pad "B12" smd rect (at -3.1 -3.05) (size 0.52 1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 41d4405e-ec9a-40c1-9eef-a9c0b6431bfc))
  (pad "S1" thru_hole oval (at -4.32 -2.675) (size 1.3 2.3) (drill oval 0.6 1.6) (layers "*.Cu" "*.Mask") (tstamp 8642eba7-d7b1-4f56-af74-4557896b198e))
  (pad "S1" thru_hole oval (at -4.32 1.15) (size 1.3 2.6) (drill oval 0.6 1.9) (layers "*.Cu" "*.Mask") (tstamp 03dea9ab-1c0f-4ef7-af93-d4d9570ce450))
  (pad "S1" thru_hole oval (at 4.32 -2.675) (size 1.3 2.3) (drill oval 0.6 1.6) (layers "*.Cu" "*.Mask") (tstamp 31286022-c900-4671-903a-c2d4cb55f4a7))
  (pad "S1" thru_hole oval (at 4.32 1.15) (size 1.3 2.6) (drill oval 0.6 1.9) (layers "*.Cu" "*.Mask") (tstamp 80edc50a-0feb-491e-a8cb-50cb0e2d19de))
  (model "${KICAD6_3DMODEL_DIR}/Connector_USB.3dshapes/USB_C_Receptacle_JAE_DX07S016JA1R1500.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
