(footprint "C_0603_HandSolder" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0 -1.2 unlocked) (layer "F.SilkS") hide
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    (tstamp e218053f-b047-408e-a386-02a4f24d3a21)
  )
  (fp_text value "C_0603_HandSolder" (at 0 1.2 unlocked) (layer "F.Fab") hide
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    (tstamp d927fcfe-7f16-4499-b318-bfda57c6048d)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
    (tstamp 7e7e4ea5-c86a-45c0-8ddf-a25fb3bfa08b)
  )
  (fp_line (start -0.1 0) (end -0.2 0)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 120eac1b-05c9-4f1f-9970-86cb81402506))
  (fp_line (start -0.1 0.2) (end -0.1 -0.2)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 01532a91-bdf7-4306-8364-80bd21d7511e))
  (fp_line (start 0.1 -0.2) (end 0.1 0.2)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0a17400b-50af-461e-811f-558743fc4fcf))
  (fp_line (start 0.1 0) (end 0.2 0)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9b998165-ee00-4a49-b6f5-2ef3e37f47a8))
  (fp_rect (start -1.6 -0.6) (end 1.6 0.6)
    (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp 6728b364-cfc5-4ad1-894b-d32f45371a8f))
  (fp_line (start -1.65 -0.73) (end 1.65 -0.73)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 14475ff7-ce8f-40c5-a019-9d8207c4ca41))
  (fp_line (start -1.65 0.73) (end -1.65 -0.73)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e5403170-9511-4b4c-8535-7d7cf0182554))
  (fp_line (start 1.65 -0.73) (end 1.65 0.73)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 60eb5ad3-5cf1-4855-af05-48ea364ab2e7))
  (fp_line (start 1.65 0.73) (end -1.65 0.73)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f9d7c337-e2f7-401c-a9e9-c5ed5707a8b7))
  (fp_line (start -0.8 -0.4) (end 0.8 -0.4)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b2b1f9d3-14a0-4556-bd3d-40618a4f3bfc))
  (fp_line (start -0.8 0.4) (end -0.8 -0.4)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2cda6e9e-6537-4827-978d-30ec95533a52))
  (fp_line (start 0.8 -0.4) (end 0.8 0.4)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 788e0366-0514-4d12-93f8-265a493aa864))
  (fp_line (start 0.8 0.4) (end -0.8 0.4)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c0dbd828-5db9-4e95-9fce-19fd61658c4e))
  (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 744e0c8e-94b2-4e98-a62f-1b666ac0e6a5))
  (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 94b7d0b0-8c47-4263-82f8-8d3130190c7d))
  (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
