(footprint "L_0603_HandSolder" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0 -1.2 unlocked) (layer "F.SilkS")
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    (tstamp 5ac12e3d-a5cc-43e7-b46e-c2fd9f0ed9c2)
  )
  (fp_text value "L_0603_HandSolder" (at 0 1.3 unlocked) (layer "F.Fab")
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    (tstamp 74538a1e-9ce6-43cf-b884-c4873d8ff48d)
  )
  (fp_text user "${REFERENCE}" (at 0 0.02) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
    (tstamp 79892c1f-f0ba-498f-b137-56b35d59557c)
  )
  (fp_rect (start -1.6 -0.58) (end 1.6 0.62)
    (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp b61ad4b5-cd23-4e5c-9c0b-7e7746be6385))
  (fp_arc (start -0.2 -0.08) (mid 0 -0.28) (end 0.2 -0.08)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3a5729fa-0efb-4d1b-8132-f67acff15c4c))
  (fp_arc (start -0.2 0.12) (mid 0 -0.08) (end 0.2 0.12)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c6c1606d-620d-4544-81b2-d8150cee08e8))
  (fp_arc (start -0.2 0.32) (mid 0 0.12) (end 0.2 0.32)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2e2347e0-76ae-457b-86c6-18d94d98c08c))
  (fp_line (start -1.65 -0.71) (end 1.65 -0.71)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b47bd5c1-a48d-4951-96db-70f67873d305))
  (fp_line (start -1.65 0.75) (end -1.65 -0.71)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ab43b911-c7b8-4568-80eb-1949f6001830))
  (fp_line (start 1.65 -0.71) (end 1.65 0.75)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5842145b-b27c-4156-a2f6-e5d090ae5dd0))
  (fp_line (start 1.65 0.75) (end -1.65 0.75)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f50a1497-3aa8-4c7d-a82c-bf968756b528))
  (fp_line (start -0.8 -0.38) (end 0.8 -0.38)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f0b99ff9-08c1-426d-92c1-9ea91d3f64e5))
  (fp_line (start -0.8 0.42) (end -0.8 -0.38)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 943e75db-af2e-4fa0-8e74-72f4fe000efb))
  (fp_line (start 0.8 -0.38) (end 0.8 0.42)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b24fdba6-962b-4d5e-a9d8-b89ac1bd67c4))
  (fp_line (start 0.8 0.42) (end -0.8 0.42)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e97d459e-c264-481b-bea3-f300bbcb22af))
  (pad "1" smd roundrect (at -0.875 0.02) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 789e8c41-b37e-44b5-80b4-12a91cf11813))
  (pad "2" smd roundrect (at 0.875 0.02) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 682c633d-c2d2-417e-b29c-3f36f3100cf0))
  (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
