(footprint "LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "5.0mm x 5.0mm Addressable RGB LED NeoPixel, https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf")
  (tags "LED RGB NeoPixel PLCC-4 5050")
  (attr smd)
  (fp_text reference "REF**" (at 0 -3.5) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 29976fa0-918e-48c1-ba81-319324267df7)
  )
  (fp_text value "LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm" (at 0 4) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 11f34c85-b80f-46bd-b71d-beeef7ef25a2)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp c5756b5f-7ccc-4d42-872b-98775daca562)
  )
  (fp_line (start -3.65 -2.75) (end 3.65 -2.75)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6ed77aa4-f296-4996-819b-3cc749559f49))
  (fp_line (start -3.65 2.75) (end 3.65 2.75)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ca1d06bb-c27e-4859-b633-e45a2345f320))
  (fp_line (start 3.65 2.75) (end 3.65 1.6)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e860fd23-f087-40be-9473-9d8e25d5ffe3))
  (fp_line (start -3.45 -2.75) (end -3.45 2.75)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e698f4d4-65a5-4d0f-a8ed-5745b8f0d483))
  (fp_line (start -3.45 2.75) (end 3.45 2.75)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 2d2813ac-2cb3-426c-9318-d6eb3fef0d3b))
  (fp_line (start 3.45 -2.75) (end -3.45 -2.75)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3ed360c1-b7ac-408f-ae9c-5f158b031e9b))
  (fp_line (start 3.45 2.75) (end 3.45 -2.75)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 62f632c6-6884-46e9-ac67-40d4696553e0))
  (fp_line (start -2.5 -2.5) (end -2.5 2.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c0c389f3-e39a-48d8-966d-313f4224879e))
  (fp_line (start -2.5 2.5) (end 2.5 2.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e4c74574-4660-4fc6-b56a-3f019923dc9c))
  (fp_line (start 2.5 -2.5) (end -2.5 -2.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e2bf95a5-2ab1-44b7-8a52-0c672195a1d4))
  (fp_line (start 2.5 1.5) (end 1.5 2.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bfb2b50f-e0ce-4bd4-b9e6-cca37d8e1b12))
  (fp_line (start 2.5 2.5) (end 2.5 -2.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 90c3ef5b-455e-4d2f-aa38-e0f89bf4bf0c))
  (fp_circle (center 0 0) (end 0 -2)
    (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 83b9b0b3-69d5-4d55-b734-61b11225d74a))
  (pad "1" smd rect (at -2.45 -1.65) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 303fa036-5e50-4d6d-bb86-5cdfd4b88a9f))
  (pad "2" smd rect (at -2.45 1.65) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 19ff1e90-56ef-461a-889c-61ffea674474))
  (pad "3" smd rect (at 2.45 1.65) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp abc776f0-6816-4443-a596-fad8645d4ac8))
  (pad "4" smd rect (at 2.45 -1.65) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp e6e3b1bc-4064-4031-9b80-d1df61337d0a))
  (model "${KICAD7_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
