(footprint "Tactile_Switch_4.2mm" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0 -2.35 unlocked) (layer "F.SilkS")
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    (tstamp de999afc-8059-46a7-ab3a-996626a7f5df)
  )
  (fp_text value "Tactile_Switch_4.2mm" (at 0 2.6 unlocked) (layer "F.Fab")
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    (tstamp 030208bf-ff57-4c29-94c3-4659767ed87f)
  )
  (fp_text user "${REFERENCE}" (at 0 4.1 unlocked) (layer "F.Fab")
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    (tstamp 9de594d7-3424-44ff-a758-dbaf82c038ee)
  )
  (fp_line (start 0 -1) (end 0 -0.5)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 8d9e8475-dd4c-4442-9e46-9795a8406924))
  (fp_line (start 0 0.5) (end -0.4 -0.5)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 9f6a9553-779b-4445-a605-664eceaa1b28))
  (fp_line (start 0 1) (end 0 0.5)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 6630f9fd-7527-447c-b158-4a7739c1e9a8))
  (fp_rect (start -2.7 -1.5) (end 2.7 1.5)
    (stroke (width 0.12) (type default)) (fill none) (layer "F.SilkS") (tstamp 014d43f9-847d-4bb1-a2d7-7784c5606f0f))
  (fp_rect (start -2.8 -1.6) (end 2.8 1.6)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp 553e50f8-cc86-4603-be9d-1c4087e3287f))
  (pad "1" smd rect (at -2.075 -1.075) (size 1.05 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 1faee6bd-8cc4-4545-a3d4-077a738bec44))
  (pad "1" smd rect (at 2.075 -1.075) (size 1.05 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 92465186-8454-474a-8395-9a21db920130))
  (pad "2" smd rect (at -2.075 1.075) (size 1.05 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 8950ec89-89d6-45ef-b068-af15bb9cf1c5))
  (pad "2" smd rect (at 2.075 1.075) (size 1.05 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 0bef0bfd-3bd6-4a6c-86ec-6629f649df37))
  (model "${KIPRJMOD}/../assets/3dmodels/PTS810 SJM 250 SMTR LFS.step"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
