(footprint "D_SOD-123" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0 -1.55 unlocked) (layer "F.SilkS")
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    (tstamp 62240be9-5a49-450d-8c43-0e7f24400280)
  )
  (fp_text value "D_SOD-123" (at 0 1.6 unlocked) (layer "F.Fab")
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    (tstamp 9056bdec-c8c0-4599-813d-8af05e5529ba)
  )
  (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab")
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    (tstamp f1db8c4c-eba7-4faf-ab42-db36cfd9a810)
  )
  (fp_line (start -2.5 -0.8) (end 2.4 -0.8)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 8abb1783-3520-4d2b-8257-e2f5435b4d4b))
  (fp_line (start -0.75 0) (end -0.35 0)
    (stroke (width 0.1) (type solid)) (layer "F.SilkS") (tstamp 5fc16b0d-3827-4c44-a750-f0c1227dc46d))
  (fp_line (start -0.35 0) (end -0.35 -0.55)
    (stroke (width 0.1) (type solid)) (layer "F.SilkS") (tstamp f7a8634e-0110-4a8b-86a4-7d631ce9de8a))
  (fp_line (start -0.35 0) (end -0.35 0.55)
    (stroke (width 0.1) (type solid)) (layer "F.SilkS") (tstamp a2896ce4-0672-4904-b05d-99209e194bdc))
  (fp_line (start -0.35 0) (end 0.25 -0.4)
    (stroke (width 0.1) (type solid)) (layer "F.SilkS") (tstamp 96fef377-6aa6-4b02-82d1-2c6e67e05258))
  (fp_line (start 0.25 -0.4) (end 0.25 0.4)
    (stroke (width 0.1) (type solid)) (layer "F.SilkS") (tstamp b6300905-ff10-4ae7-be1f-4e72f4dd64a7))
  (fp_line (start 0.25 0) (end 0.75 0)
    (stroke (width 0.1) (type solid)) (layer "F.SilkS") (tstamp 150bf176-551e-4192-ab65-eb9fb8d2074e))
  (fp_line (start 0.25 0.4) (end -0.35 0)
    (stroke (width 0.1) (type solid)) (layer "F.SilkS") (tstamp f2616fb9-c7a1-4456-a9a9-e0b5b64416f8))
  (fp_line (start 2.4 -0.8) (end 2.4 0.8)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp cfb7fb8a-daa9-4ee1-bfa4-def5db9348b2))
  (fp_line (start 2.4 0.8) (end -2.5 0.8)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 798493c3-21ed-43c2-adb4-3e73f2552aab))
  (fp_rect (start -2.5 -0.8) (end -2.3 0.8)
    (stroke (width 0.12) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 323bda46-1972-4321-908e-ed226e221a80))
  (fp_rect (start -2.45 -1.16) (end 2.47 1.16)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp d586f0ed-5baf-4950-b24d-de65856a7f11))
  (fp_line (start -2.35 -0.82) (end -2.35 0.8)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 2a6f28a1-f3d5-4c7f-bf12-79a15a081039))
  (fp_line (start -1.6 -1.05) (end -1.6 1.05)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp ae5792a8-ae5d-4c66-8039-db6f1174e32d))
  (fp_line (start -1.6 -1.05) (end 1.6 -1.05)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 949d416a-2ac6-4551-b041-e1c17c75bb85))
  (fp_line (start -1.6 -0.82) (end -2.35 -0.82)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 0db9aa21-efbf-49b0-a02e-e7d2f9d40ff4))
  (fp_line (start -1.6 0.8) (end -2.35 0.8)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 16938ae7-02d0-4553-9060-6d7eb15bf0ef))
  (fp_line (start -1.6 1.05) (end 1.6 1.05)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 88b2c524-3930-4e02-b584-fcd5f9abdd75))
  (fp_line (start 1.6 -1.05) (end 1.6 1.05)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 6f2cf60e-79b5-40b5-a92c-66b28481dc98))
  (fp_line (start 1.6 -0.81) (end 2.35 -0.81)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 2943e36d-192a-40ac-bbd0-35b0e8c4ebc0))
  (fp_line (start 1.6 0.81) (end 2.35 0.81)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 1575aedf-1e49-4c0e-ba1d-8c62ac19dc15))
  (fp_line (start 2.35 -0.81) (end 2.35 0.81)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 8460211a-0396-445e-a41e-810d8e66e9d5))
  (pad "1" smd rect (at -1.635 0) (size 0.91 1.22) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 83fc256d-8481-4b77-8301-30941af5fece))
  (pad "2" smd rect (at 1.635 0) (size 0.91 1.22) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp a4088b54-1202-4be8-a656-376952a434d1))
  (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
