(footprint "LED_0805_LiteOn" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0 -1.5 unlocked) (layer "F.SilkS")
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    (tstamp 19aebe8e-4730-42c1-bdbb-42da14878e91)
  )
  (fp_text value "LED_0805_LiteOn" (at 0 2.85 unlocked) (layer "F.Fab")
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    (tstamp f77c3edb-ff94-44e9-a565-cbf16001dddc)
  )
  (fp_text user "${REFERENCE}" (at 0 1.65 unlocked) (layer "F.Fab")
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    (tstamp 66ffcb97-1d24-4e8d-bf9d-e35c888fbbfa)
  )
  (fp_line (start -2.2 -0.9) (end 2 -0.9)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 9f2ca89b-deb6-4ea6-b527-183be4ea9946))
  (fp_line (start -0.35 0) (end 0.25 -0.3)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ebf08ff6-c014-4eab-b7af-e2a71d9b464d))
  (fp_line (start -0.35 0.3) (end -0.35 -0.3)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9537b722-3b56-4ee8-b8f8-0e4447f530f8))
  (fp_line (start 0.25 -0.3) (end 0.25 0.3)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 00903012-e6cf-4bd5-b6ce-58aa3f33deee))
  (fp_line (start 0.25 0.3) (end -0.35 0)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 77130769-4605-4695-8173-7d658e432473))
  (fp_line (start 2 -0.9) (end 2 0.9)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp a1e40d0d-bbe6-4894-9567-09a4a2fb1f32))
  (fp_line (start 2 0.9) (end -2.2 0.9)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp ed4595f9-4a46-4eca-8079-bea99f34ef73))
  (fp_rect (start -2.2 -0.9) (end -2 0.9)
    (stroke (width 0.12) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 9f33c265-d35c-4632-8f71-0bee58eb09a9))
  (fp_rect (start -2.15 -1) (end 2.1 1)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp 77f0cd38-e08c-447a-9e34-78604f081ed0))
  (fp_rect (start -1.3 -0.7) (end 1.3 0.7)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp c9d076c2-0f10-4d03-9e12-ccb91c81acb1))
  (pad "1" smd rect (at -1.25 0) (size 1.1 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp ad925907-930f-4585-b421-b7f02345e6e0))
  (pad "2" smd rect (at 1.25 0) (size 1.1 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 690b40a1-0c6f-4eb1-bdea-417c63fe3738))
  (model "/home/cynt4k-emgenics/Documents/Privat/pcb-droid/hardware/pcbs/assets/3dmodels/LTST-C171KRKT.stp"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
