(footprint "RP2040_QFN-56" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 4.4 -4.35 90) (layer "F.SilkS")
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    (tstamp 2e16eeea-7da9-46e8-a459-a683ca28fb99)
  )
  (fp_text value "RP2040_QFN-56" (at 0 5.2) (layer "F.Fab")
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    (tstamp daefd63f-c53c-4112-b905-39b485842eff)
  )
  (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab") hide
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    (tstamp a88e8935-3e50-4ef7-b297-04de49edffc5)
  )
  (fp_line (start -3.61 3.61) (end -3.61 2.96)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 767e0cab-345e-425c-9bee-b159dddc9dba))
  (fp_line (start -2.96 -3.61) (end -3.61 -3.61)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp cdba5143-1ee1-4d5d-bbae-06fa910f4c7d))
  (fp_line (start -2.96 3.61) (end -3.61 3.61)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 35ca30bd-b4af-43eb-be9d-18b8db9f506d))
  (fp_line (start 2.96 -3.61) (end 3.61 -3.61)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp dfe7b60d-edb8-47e4-8072-c9fb9148c9df))
  (fp_line (start 2.96 3.61) (end 3.61 3.61)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5d770687-38fb-4aa9-916d-83033777afe0))
  (fp_line (start 3.61 -3.61) (end 3.61 -2.96)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9fcfd433-d262-41f2-9147-bbc77de6afd4))
  (fp_line (start 3.61 3.61) (end 3.61 2.96)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 147fd5cf-0d04-43aa-b5ab-eb785ab7b4ff))
  (fp_circle (center -4.5 -3.1) (end -4.052786 -3.1)
    (stroke (width 0.12) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 529fcccf-bd79-4a55-b14d-8f1f2353c7a1))
  (fp_line (start -4.12 -4.12) (end -4.12 4.12)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 177caa9d-6a1a-4e50-b998-456db95cb59e))
  (fp_line (start -4.12 4.12) (end 4.12 4.12)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3bf930d1-473e-4d31-8793-6cb0ee15e724))
  (fp_line (start 4.12 -4.12) (end -4.12 -4.12)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 059cbe92-0903-4010-815e-c347a9d661c3))
  (fp_line (start 4.12 4.12) (end 4.12 -4.12)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 45edf996-d86c-4616-959b-a4f93f48fb8a))
  (fp_line (start -3.5 -2.5) (end -2.5 -3.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 95d40197-3cab-4418-9d8b-bd81daac2065))
  (fp_line (start -3.5 3.5) (end -3.5 -2.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp eb2a2af0-cc53-47aa-806e-f3a657c0312d))
  (fp_line (start -2.5 -3.5) (end 3.5 -3.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 412efc37-d4c8-48be-a828-6889f4889e45))
  (fp_line (start 3.5 -3.5) (end 3.5 3.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 69750add-de0a-4b91-a821-470ad6a1ebeb))
  (fp_line (start 3.5 3.5) (end -3.5 3.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 76279168-4f14-442f-9c0b-f81aa7fb097f))
  (pad "" smd roundrect (at -0.6375 -0.6375) (size 1.084435 1.084435) (layers "F.Paste") (roundrect_rratio 0.2305347946) (tstamp 80e979c4-87fd-47de-bbb4-9d73a7692143))
  (pad "" smd roundrect (at -0.6375 0.6375) (size 1.084435 1.084435) (layers "F.Paste") (roundrect_rratio 0.2305347946) (tstamp 3259b57e-e20e-422f-a46b-5e8d9687c25a))
  (pad "" smd roundrect (at 0.6375 -0.6375) (size 1.084435 1.084435) (layers "F.Paste") (roundrect_rratio 0.2305347946) (tstamp 588a2ffd-2879-4135-a9ce-4593627f62d5))
  (pad "" smd roundrect (at 0.6375 0.6375) (size 1.084435 1.084435) (layers "F.Paste") (roundrect_rratio 0.2305347946) (tstamp d6b7e11d-390c-4052-8e2e-40f3b5f0c790))
  (pad "1" smd roundrect (at -3.4375 -2.6) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 9b23d692-dc4c-4934-8704-6f0a4c629fb7))
  (pad "2" smd roundrect (at -3.4375 -2.2) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 84b06418-f02c-43ed-9ff3-81672773f9d3))
  (pad "3" smd roundrect (at -3.4375 -1.8) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp f687eadb-0f4d-42e0-8c53-14083921d30d))
  (pad "4" smd roundrect (at -3.4375 -1.4) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 784c95cb-202e-4e7f-8854-4a4e52b70161))
  (pad "5" smd roundrect (at -3.4375 -1) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 84466c16-d1fa-4594-adb4-3a0c75699f67))
  (pad "6" smd roundrect (at -3.4375 -0.6) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp d3a19cf2-3ed9-41de-9a3f-1b468e31089e))
  (pad "7" smd roundrect (at -3.4375 -0.2) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 4db73c4e-4eea-463c-ad9b-953a3eb2ce31))
  (pad "8" smd roundrect (at -3.4375 0.2) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp f559299d-35e1-4b00-addf-4a54b921c70c))
  (pad "9" smd roundrect (at -3.4375 0.6) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp a8a2a79a-96e2-48a7-9e48-1da2bacc79ca))
  (pad "10" smd roundrect (at -3.4375 1) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 5f99cf07-c9bc-49e9-b0b7-51d2dd115b28))
  (pad "11" smd roundrect (at -3.4375 1.4) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 147a8d7e-4c68-448c-900e-94160cee882d))
  (pad "12" smd roundrect (at -3.4375 1.8) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 61c777a3-1814-41aa-9477-af8950e49fec))
  (pad "13" smd roundrect (at -3.4375 2.2) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 5204ba19-cb57-4ac4-b419-403042f33a6d))
  (pad "14" smd roundrect (at -3.4375 2.6) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp e30a1f70-0034-4930-855d-9724b03ad3d4))
  (pad "15" smd roundrect (at -2.6 3.4375) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 09130b3c-ef0f-4427-b304-3004f85353f6))
  (pad "16" smd roundrect (at -2.2 3.4375) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 45ff3886-226c-49a4-b842-485e7bb30f77))
  (pad "17" smd roundrect (at -1.8 3.4375) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 89ca5b1b-e7f8-4989-aaab-8660effb87c5))
  (pad "18" smd roundrect (at -1.4 3.4375) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 4bf7b1a2-d2a4-4ded-87cd-71fb96812c2d))
  (pad "19" smd roundrect (at -1 3.4375) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp e350f64a-7ee8-4758-8662-de5ede3432da))
  (pad "20" smd roundrect (at -0.6 3.4375) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp f00725da-4cc3-4f91-a644-0004518e7901))
  (pad "21" smd roundrect (at -0.2 3.4375) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 77fe0f01-1c30-4b6e-99e5-4551381e9277))
  (pad "22" smd roundrect (at 0.2 3.4375) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 8620a259-0cf6-4418-92c1-2b0bd35ceda7))
  (pad "23" smd roundrect (at 0.6 3.4375) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp f285b40d-8ca6-43e2-a575-e80be1081b08))
  (pad "24" smd roundrect (at 1 3.4375) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 68fa4959-80f2-4d8c-b1ec-76247547cc2c))
  (pad "25" smd roundrect (at 1.4 3.4375) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 038e62b3-7eff-4d70-8bcf-e13ee22789c3))
  (pad "26" smd roundrect (at 1.8 3.4375) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp d86f0f29-ff9e-4c40-ba01-8fb52e160501))
  (pad "27" smd roundrect (at 2.2 3.4375) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp c1f77920-5589-4f6a-aa84-e2b1510b5828))
  (pad "28" smd roundrect (at 2.6 3.4375) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 05603042-f659-42db-b37c-55a794d5d13c))
  (pad "29" smd roundrect (at 3.4375 2.6) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp ae70f554-d11d-45c6-b3c7-928f0d7d2a40))
  (pad "30" smd roundrect (at 3.4375 2.2) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp f4711c65-1a2b-49c9-8bf5-1e83723b97d6))
  (pad "31" smd roundrect (at 3.4375 1.8) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 22632565-7a4d-44bb-ad36-e894f88a61ce))
  (pad "32" smd roundrect (at 3.4375 1.4) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp a8ba6e0a-8b0a-42c4-8984-77075b10a5ef))
  (pad "33" smd roundrect (at 3.4375 1) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp b8643292-97d6-4031-8106-a9e66f67e9c5))
  (pad "34" smd roundrect (at 3.4375 0.6) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 6e0f1876-3bcf-46c4-a90a-b120f3ff7188))
  (pad "35" smd roundrect (at 3.4375 0.2) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 41dedfba-38f7-4064-ba8b-be737d379a36))
  (pad "36" smd roundrect (at 3.4375 -0.2) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp c71d3463-7ee2-4776-b4d3-d9cf0a98e828))
  (pad "37" smd roundrect (at 3.4375 -0.6) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 6c65b490-9fdd-413c-922b-465ff837a7da))
  (pad "38" smd roundrect (at 3.4375 -1) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 32aa9b2d-6ec0-4be5-a90c-a2b724d26dd7))
  (pad "39" smd roundrect (at 3.4375 -1.4) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp d3797c5a-1302-4b6c-9296-5bba57e637eb))
  (pad "40" smd roundrect (at 3.4375 -1.8) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 71c55688-a307-4541-a01c-66bb722b90ac))
  (pad "41" smd roundrect (at 3.4375 -2.2) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp fedcfd19-e492-438d-b57b-79d28d186725))
  (pad "42" smd roundrect (at 3.4375 -2.6) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp bdb8d698-dd6c-4852-8d8d-17b7071f36c4))
  (pad "43" smd roundrect (at 2.6 -3.4375) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 8a35b261-fbe5-4e77-a57d-e2a5aff0c681))
  (pad "44" smd roundrect (at 2.2 -3.4375) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 211b9e20-c993-4093-9ab5-186ba6c98a3a))
  (pad "45" smd roundrect (at 1.8 -3.4375) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp e4b1cd27-a4d1-4bef-bae5-631df945b1f7))
  (pad "46" smd roundrect (at 1.4 -3.4375) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp b88ecb3c-cbff-472f-8e09-b8fa3f46646f))
  (pad "47" smd roundrect (at 1 -3.4375) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 6425bb74-c639-4b17-810c-b7695ecd6b6e))
  (pad "48" smd roundrect (at 0.6 -3.4375) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 3504140c-3342-4d8a-a7d5-a701d66be3d1))
  (pad "49" smd roundrect (at 0.2 -3.4375) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp e750f1b5-6f5c-4f88-876b-0412d66ac948))
  (pad "50" smd roundrect (at -0.2 -3.4375) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 31b1cd2b-df85-49de-a297-fbdcd48e66c1))
  (pad "51" smd roundrect (at -0.6 -3.4375) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp cb9570df-0081-46af-adcd-eadc1997e262))
  (pad "52" smd roundrect (at -1 -3.4375) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp fffb942e-6771-470a-b484-1eb7bed96311))
  (pad "53" smd roundrect (at -1.4 -3.4375) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp a1d04178-bcce-46b3-b7f2-65211f64dd32))
  (pad "54" smd roundrect (at -1.8 -3.4375) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp b9776f59-fa11-4e77-a572-6909b1125196))
  (pad "55" smd roundrect (at -2.2 -3.4375) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp a84b4c62-0063-4903-8fe0-9db90403652f))
  (pad "56" smd roundrect (at -2.6 -3.4375) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 62393902-d974-4f11-bde4-b76d30e8d94a))
  (pad "57" smd roundrect (at 0 0) (size 3.2 3.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.045) (tstamp 81419d8a-2b5a-4111-905a-90f9bf20db7f))
  (model "${KIPRJMOD}/../assets/3dmodels/SC0914_7.stp"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
