(footprint "C_0805_HandSolder" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
  (tags "capacitor handsolder")
  (attr smd)
  (fp_text reference "REF**" (at 0 -1.68) (layer "F.SilkS")
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    (tstamp 79648a8a-db92-4d15-88fe-c63b15560e19)
  )
  (fp_text value "C_0805_HandSolder" (at 0 1.68) (layer "F.Fab")
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    (tstamp 2faa6533-bd7f-4045-b3e8-f0563d8bdcb0)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    (tstamp 2aa51584-7f2e-4a4a-b57d-bfb466824e30)
  )
  (fp_line (start -0.1 -0.2) (end -0.1 0.2)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ae0970a7-9b24-4fc8-b4fe-4202e54e4dd4))
  (fp_line (start -0.1 0) (end -0.3 0)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp bc41ad9b-214f-4e69-95c2-fd90ef8b39a4))
  (fp_line (start 0.1 -0.2) (end 0.1 0.2)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6440c980-06a6-46d7-bb0e-fb589f1e53ce))
  (fp_line (start 0.1 0) (end 0.3 0)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f9b62a64-a54d-455f-93b1-f5f77146cf92))
  (fp_rect (start -1.8 -0.9) (end 1.8 0.9)
    (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp 9e302d14-9164-4843-94a8-14250c4e287f))
  (fp_line (start -1.88 -0.98) (end 1.88 -0.98)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f6be3644-2a54-4fbf-bf15-5b6eed6d8a56))
  (fp_line (start -1.88 0.98) (end -1.88 -0.98)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c529675f-a8ed-44d1-80ae-ea250a6903d7))
  (fp_line (start 1.88 -0.98) (end 1.88 0.98)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 54dff31b-cb37-4ff9-b6c6-2a622ddda3ef))
  (fp_line (start 1.88 0.98) (end -1.88 0.98)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 48d7958a-7eb3-477d-82cc-d56aca09968e))
  (fp_line (start -1 -0.625) (end 1 -0.625)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 462dcbaa-110b-4c22-b113-3e85baeea0e0))
  (fp_line (start -1 0.625) (end -1 -0.625)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c27546ee-1d07-4d96-bdd5-078fe9468528))
  (fp_line (start 1 -0.625) (end 1 0.625)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7c9750b1-41ff-4bba-a611-82cfc4e49440))
  (fp_line (start 1 0.625) (end -1 0.625)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bfbad6ed-9bbd-4a1a-bdfe-ee50245a621a))
  (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766) (tstamp 5c952ec8-c980-4a94-a972-30f730128869))
  (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766) (tstamp 26b8f07a-78fd-4334-a627-c22ac9be221b))
  (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
