(footprint "JST_SH_SM03B-SRSS-TB_1x03-1MP_P1.00mm_Horizontal" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "JST SH series connector, SM03B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
  (tags "connector JST SH top entry")
  (attr smd)
  (fp_text reference "REF**" (at 0 -3.98) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 6528759d-c307-4b38-ad59-2c627fff9226)
  )
  (fp_text value "JST_SH_SM03B-SRSS-TB_1x03-1MP_P1.00mm_Horizontal" (at 0 3.98) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp f21dc044-8bed-47ad-a3ca-aa19af5133eb)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp d55a8d66-4275-4234-a2b9-63388826156c)
  )
  (fp_line (start -2.61 -1.785) (end -1.56 -1.785)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 771d31aa-f7a9-43be-8179-cd94bfa5f3d7))
  (fp_line (start -2.61 0.715) (end -2.61 -1.785)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a1ebfbf9-352d-478d-ae32-6c47ebbf7952))
  (fp_line (start -1.56 -1.785) (end -1.56 -2.775)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b9797a82-1ae9-468f-98d0-c089851f3e00))
  (fp_line (start -1.44 2.685) (end 1.44 2.685)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4b204828-4fae-42db-b613-0740f7359d2a))
  (fp_line (start 2.61 -1.785) (end 1.56 -1.785)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5f440c4f-51cf-4436-bd27-554d3985ee4f))
  (fp_line (start 2.61 0.715) (end 2.61 -1.785)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c34c47d7-13b9-4b64-8a0e-f1fb992fa74d))
  (fp_line (start -3.4 -3.28) (end -3.4 3.28)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 90e288a9-648e-4cfd-82d9-da86db43726a))
  (fp_line (start -3.4 3.28) (end 3.4 3.28)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 64d4c782-f2f8-4d11-9c44-eba6b3fa22b3))
  (fp_line (start 3.4 -3.28) (end -3.4 -3.28)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8f5d1a91-d16d-4eb9-aeae-c3709d19f391))
  (fp_line (start 3.4 3.28) (end 3.4 -3.28)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8e717b9e-7ecf-4a77-aefb-4f6a31f7a985))
  (fp_line (start -2.5 -1.675) (end -2.5 2.575)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5a4a31db-1381-4772-b5de-fa414979a793))
  (fp_line (start -2.5 -1.675) (end 2.5 -1.675)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b6993c77-8dee-4b82-bbf3-0629fdb470f2))
  (fp_line (start -2.5 2.575) (end 2.5 2.575)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 92216a6d-8f63-4771-bec8-1805e9a3488e))
  (fp_line (start -1.5 -1.675) (end -1 -0.967893)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp dc19ab2c-90d0-49f0-b381-c2962f2e99e8))
  (fp_line (start -1 -0.967893) (end -0.5 -1.675)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 18ac3b15-46fd-4bca-8884-6ac7a2071db5))
  (fp_line (start 2.5 -1.675) (end 2.5 2.575)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 673eec34-21f8-4bd8-9af1-8063af7a996c))
  (pad "1" smd roundrect (at -1 -2) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp cf415d1c-9e1a-4b11-8eba-ec7c9361d97a))
  (pad "2" smd roundrect (at 0 -2) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 00d27945-4923-479a-961c-b6c23c95466b))
  (pad "3" smd roundrect (at 1 -2) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp d2971d40-1075-4baa-92b9-907e96b4a68e))
  (pad "MP" smd roundrect (at -2.3 1.875) (size 1.2 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333) (tstamp af9dfdde-ffe5-4b67-bbbb-7ed1b905e3bb))
  (pad "MP" smd roundrect (at 2.3 1.875) (size 1.2 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333) (tstamp 0a8636a3-3fac-4e8d-9226-a1208b6d6572))
  (model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_SH_SM03B-SRSS-TB_1x03-1MP_P1.00mm_Horizontal.wrl"
    (offset (xyz 0 1.3 -0.4))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
