(footprint "D_SMA" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0 -2.5 unlocked) (layer "F.SilkS")
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    (tstamp 101dd83d-e273-43b2-9066-fe023113bb85)
  )
  (fp_text value "D_SMA" (at 0 2.5 unlocked) (layer "F.Fab")
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    (tstamp 5a0cade9-bbf6-41f2-8986-9000dc1c177d)
  )
  (fp_text user "${REFERENCE}" (at 0 -2.4 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp edc7461e-e421-4dd2-8c6e-c1da9fe56646)
  )
  (fp_line (start -3.65 1.6) (end 3.4 1.6)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp cf697556-e4e7-4910-acf6-60ee6779ab31))
  (fp_line (start -0.55 0) (end -0.3 0)
    (stroke (width 0.1) (type solid)) (layer "F.SilkS") (tstamp a21088e3-6e8b-4a36-8493-9a30b3f7b8dc))
  (fp_line (start -0.3 0) (end -0.3 -0.55)
    (stroke (width 0.1) (type solid)) (layer "F.SilkS") (tstamp 02c3cf0b-4338-4a44-b5a1-6f1c831153b4))
  (fp_line (start -0.3 0) (end -0.3 0.55)
    (stroke (width 0.1) (type solid)) (layer "F.SilkS") (tstamp 75ea920f-7eba-4939-8741-851ef7d7ac8f))
  (fp_line (start 0.3 0) (end 0.55 0)
    (stroke (width 0.1) (type solid)) (layer "F.SilkS") (tstamp d69a4458-810a-430d-915b-4e6c7520dd02))
  (fp_line (start 3.4 -1.6) (end -3.65 -1.6)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp bf565f2d-caa3-4b98-91e5-21af7c6c768a))
  (fp_line (start 3.4 -1.6) (end 3.4 1.6)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp be802c4f-bc90-4dd9-ad3a-61a4eab1d1fa))
  (fp_rect (start -3.65 -1.6) (end -3.35 1.6)
    (stroke (width 0.12) (type solid)) (fill solid) (layer "F.SilkS") (tstamp a47db964-270b-4ec3-9ae6-ac86d15a7c87))
  (fp_poly
    (pts
      (xy 0.3 0.4)
      (xy -0.3 0)
      (xy 0.3 -0.4)
    )

    (stroke (width 0.12) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 916c1554-73ca-4948-ab2f-407899f8d807))
  (fp_rect (start -3.75 -1.7) (end 3.5 1.7)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp 16992299-766a-4078-8db3-dd95dc4e6b59))
  (fp_line (start -0.6 -0.8) (end -0.6 0.8)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 7185c7c6-1b92-4edf-8f6d-299110b5183a))
  (fp_line (start -0.6 0) (end -1.4 0)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp a040f226-196b-4f47-8818-d0a33a59860c))
  (fp_line (start -0.6 0) (end 0.6 0.8)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp b08a3a7e-e0fd-4fdd-a9c6-2abb45bf236e))
  (fp_line (start 0.6 -0.8) (end -0.6 0)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 402fcc71-35fb-4b45-90ef-4242acd20807))
  (fp_line (start 0.6 0) (end 0.6 -0.8)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp a3ec51e0-4c3d-49af-9e2d-f0ac28b8fb52))
  (fp_line (start 0.6 0.8) (end 0.6 0)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 84e5a1db-b0ab-4102-a6fa-9f2a13cf823f))
  (fp_line (start 1.4 0) (end 0.6 0)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 91120b4f-073d-4b9f-868f-9986e5f9c6cf))
  (fp_rect (start -2.3 -1.4) (end 2.3 1.4)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp b804c9d1-c902-4749-9aff-24ed09ff0dce))
  (pad "1" smd rect (at -1.95 0.05) (size 2.5 2.5) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 7f0b57a4-f0b0-4263-aee4-99be05b76dbf))
  (pad "2" smd rect (at 1.95 0) (size 2.5 2.5) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 86660744-6126-4cc3-b07a-df254f93a843))
  (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
