(footprint "Cryrstal_SMD_ABRACON_ABMM-4Pin_7.0x5.0mm" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0 -3.45 unlocked) (layer "F.SilkS")
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    (tstamp a7bf8da0-df4f-46b1-9e36-99c249166ccd)
  )
  (fp_text value "Cryrstal_SMD_ABRACON_ABMM-4Pin_7.0x5.0mm" (at 0 3.6 unlocked) (layer "F.Fab")
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    (tstamp 9d29b3f8-2689-4156-88b3-aeebc7844ef5)
  )
  (fp_text user "${REFERENCE}" (at 0 4.95 unlocked) (layer "F.Fab")
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    (tstamp dd7fed25-c2bd-44c6-868a-e01bc926fc88)
  )
  (fp_line (start -4.2 0.3) (end -3.7 0.3)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7356ff7a-4f12-476f-bdfd-a7b896303bd3))
  (fp_line (start -4.2 2.4) (end -3.7 2.4)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp acf2fed7-96c9-48a6-a600-aaa133d490f0))
  (fp_line (start -3.7 -2.7) (end 3.7 -2.7)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8b095ab3-e1e7-4715-841a-4dbc691bad01))
  (fp_line (start -3.7 -2.4) (end -3.7 -2.7)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 456b208d-3220-4621-8db0-51bd151362f1))
  (fp_line (start -3.7 0.3) (end -3.7 -0.3)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d89766cf-c502-4be3-bea9-a8d23a8c26e6))
  (fp_line (start -3.7 2.4) (end -3.7 2.7)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 896b561d-1506-4d74-a33a-321653ca98d2))
  (fp_line (start -3.7 2.7) (end 3.7 2.7)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6c87ef11-7b43-46e8-88a4-40a9edf23836))
  (fp_line (start 3.7 -2.7) (end 3.7 -2.4)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 98991e33-2385-4bb3-953d-7f8d81b84159))
  (fp_line (start 3.7 -0.3) (end 3.7 0.3)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 366075bb-d361-438c-8e19-5580c98e091a))
  (fp_line (start 3.7 2.7) (end 3.7 2.4)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 47d2beae-81b5-4a05-909b-a836fb51767e))
  (fp_line (start -4.3 -2.8) (end -4.3 2.8)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a4696688-a1e0-45a7-8a9e-760dccb79540))
  (fp_line (start -4.3 2.8) (end 4.3 2.8)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8574bc80-8d00-4670-bb94-6f5760ccd7cd))
  (fp_line (start 4.3 -2.8) (end -4.3 -2.8)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 56c484d7-2a12-48c4-9563-7f65f6f1e490))
  (fp_line (start 4.3 2.8) (end 4.3 -2.8)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 345b58f2-8174-4ba5-8afb-20c2ee0db67b))
  (fp_line (start -3.5 -2.3) (end -3.3 -2.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bc50b5bf-0570-4d2d-8dc1-ccc27f100ce3))
  (fp_line (start -3.5 1.5) (end -2.5 2.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8b655519-a59c-4bf6-9739-3b5581211b6c))
  (fp_line (start -3.5 2.3) (end -3.5 -2.3)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bdb93a3b-15db-46c6-afe0-7dc4a46e99d9))
  (fp_line (start -3.3 -2.5) (end 3.3 -2.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 056ceb9e-1b4b-49dd-bb8d-3a3777efb17c))
  (fp_line (start -3.3 2.5) (end -3.5 2.3)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ec17d639-a573-4976-adfc-d4cd82affd98))
  (fp_line (start 3.3 -2.5) (end 3.5 -2.3)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 91886cb8-bb47-4c24-9f85-cbac6397859c))
  (fp_line (start 3.3 2.5) (end -3.3 2.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 48969820-afa8-45fe-b13c-6b0be06ef305))
  (fp_line (start 3.5 -2.3) (end 3.5 2.3)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9985dde3-cf71-4abb-901a-cfb0b3667044))
  (fp_line (start 3.5 2.3) (end 3.3 2.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e3ac1dc7-3b3b-48b8-ad33-952523e3fccc))
  (pad "1" smd rect (at -2.95 1.35) (size 2.1 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 268d2609-ecca-4ad0-ba84-e4cf387a29d0))
  (pad "2" smd rect (at -2.95 -1.35) (size 2.1 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 6a427fd3-d54a-4141-a6a4-291901f57d62))
  (pad "3" smd rect (at 2.95 -1.35) (size 2.1 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 254985c9-1871-476a-9f39-73e9c7171a15))
  (pad "4" smd rect (at 2.95 1.35) (size 2.1 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 60bb050c-3a53-4343-ba53-7e29d2356094))
  (model "${KIPRJMOD}/../assets/3dmodels/ABMM-12.000MHZ-B2.STEP"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
