(footprint "APB2LAN_SMT" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0.05 -4.9 unlocked) (layer "F.SilkS")
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    (tstamp 1dcd6012-d15c-40ff-a979-66eadcddadb7)
  )
  (fp_text value "APB2LAN_SMT" (at 0 5.35 unlocked) (layer "F.Fab")
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    (tstamp 6180205b-6add-403f-ba82-d72db197c733)
  )
  (fp_text user "${REFERENCE}" (at 0 6.85 unlocked) (layer "F.Fab")
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    (tstamp 3ce0ef0b-335b-44c3-8ced-42cecb8c0b9d)
  )
  (fp_rect (start -3.6 -4.1) (end 3.6 4.1)
    (stroke (width 0.12) (type default)) (fill none) (layer "F.SilkS") (tstamp 0a6f860a-c5fc-4fdf-8a09-4f1b5d296a4d))
  (fp_circle (center -4 4.45) (end -3.8 4.45)
    (stroke (width 0.12) (type solid)) (fill solid) (layer "F.SilkS") (tstamp e8a69945-e4fe-4eda-b5af-177a17043221))
  (fp_rect (start -3.7 -4.2) (end 3.7 4.2)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp 709f4af0-f35c-4e9a-a971-afe0999291a7))
  (pad "1" smd rect (at -2.35 2.5) (size 1.95 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 5d9383b5-3537-49c7-b9b5-8a37e2d79919))
  (pad "2" smd rect (at -2.35 0) (size 1.95 1.45) (layers "F.Cu" "F.Paste" "F.Mask" "Eco2.User") (tstamp 786d53c6-63dd-4b56-9b5a-8e770b9712e8))
  (pad "3" smd rect (at -2.35 -2.5) (size 1.95 1.45) (layers "F.Cu" "F.Paste" "F.Mask" "Eco2.User") (tstamp cbb9fb3d-c98c-4cf8-a7a9-f654d00571fc))
  (pad "4" smd rect (at 2.35 -2.5) (size 1.95 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp e6a6159e-4230-48cf-921d-018d08962f37))
  (pad "5" smd rect (at 2.35 0) (size 1.95 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 0564cde7-4e54-46cb-afdf-e96baa87661f))
  (pad "6" smd rect (at 2.35 2.5) (size 1.95 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp f4778056-a2e3-4d03-bab7-bde616fcb5c3))
  (model "${KIPRJMOD}/../assets/3dmodels/honeywell-abp2-series-32347845-001_sw_a.stp"
    (offset (xyz -6.15 -6.5 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
