(footprint "TerminalBlock_PhoenixContact_2x5mm" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -5.3 unlocked) (layer "F.SilkS")
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    (tstamp 962f0a64-0cf1-41d1-94aa-3013d0ca6c62)
  )
  (fp_text value "TerminalBlock_PhoenixContact_2x5mm" (at 0 5.3 unlocked) (layer "F.Fab")
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    (tstamp 5f09990c-0bae-4720-a33f-7459c2966c2b)
  )
  (fp_text user "${REFERENCE}" (at 0 6.6 unlocked) (layer "F.Fab")
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    (tstamp ac9e6c18-6ef5-4013-816e-a48467481487)
  )
  (fp_line (start -4.3 -1) (end -4.3 1)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 06e3c4e5-7de2-4261-9a66-e61fc8a6133b))
  (fp_line (start -3.5 -1.8) (end -1.5 -1.8)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 61edb6d6-72c8-450a-b903-7bc970bf3f72))
  (fp_line (start -3.5 1.8) (end -1.5 1.8)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ff5d9b73-724f-43d2-a616-6a849b5426c1))
  (fp_line (start -0.7 -1) (end -0.7 1)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ddc925c8-eeb7-41ed-a5e5-4aa14e2ddada))
  (fp_rect (start -5 -4.15) (end 5 -3.65)
    (stroke (width 0.12) (type solid)) (fill solid) (layer "F.SilkS") (tstamp cc9af439-7f5b-4b76-97a9-52b4cf213338))
  (fp_rect (start -5 -4.15) (end 5 4.15)
    (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp c4f33599-faa1-47f0-b807-f839951ada36))
  (fp_arc (start -4.3 -1) (mid -4.065685 -1.565685) (end -3.5 -1.8)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 99c18695-2963-4bb9-90ff-0a578b9f1eb3))
  (fp_arc (start -3.5 1.8) (mid -4.065685 1.565685) (end -4.3 1)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7563b446-cfd7-4eba-af33-d1b6c7ff9a3d))
  (fp_arc (start -1.5 -1.8) (mid -0.934315 -1.565685) (end -0.7 -1)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7d9c5f8a-803a-403d-a843-ca9e0fe2b584))
  (fp_arc (start -0.7 1) (mid -0.934315 1.565685) (end -1.5 1.8)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp bb42aa6a-2f60-40b7-bf9a-b132c2279a06))
  (fp_circle (center 2.5 0) (end 3.9 1.2)
    (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp 0e074c3c-e2c4-472d-92a3-fb76c1175349))
  (fp_poly
    (pts
      (xy -1.603852 4.136426)
      (xy -3.453852 4.136426)
      (xy -2.503852 2.586426)
    )

    (stroke (width 0.12) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 9aadbcf6-48d4-4a15-88dd-00f60446cd74))
  (fp_poly
    (pts
      (xy 3.3865 4.13786)
      (xy 1.5365 4.13786)
      (xy 2.4865 2.58786)
    )

    (stroke (width 0.12) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 464c7c42-6848-4143-960b-2fd5ce2fc47f))
  (fp_rect (start -5.5 -4.5) (end 5.5 4.5)
    (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp bff991c2-6d1e-4e78-a921-6374a1a24c7a))
  (fp_rect (start -5 -4.15) (end 5 4.15)
    (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 2ef4c436-f8e2-40f9-be43-8eb7358071a4))
  (fp_rect (start -3.45 4.15) (end -1.55 2.45)
    (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 973bc1a5-f775-43a0-9335-fcb952980d8c))
  (fp_rect (start -3 -0.45) (end -2 0.55)
    (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 36450e94-4a8e-413f-a3a9-a1dbd583cce2))
  (fp_rect (start 1.5 2.45) (end 3.4 4.15)
    (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 45aafe97-5cea-48b2-a0b7-3d43f5369d3d))
  (fp_rect (start 2 -0.45) (end 3 0.55)
    (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 7b962b5d-73df-45e4-a462-4aeea721e6fe))
  (pad "1" thru_hole roundrect (at -2.5 0) (size 2.8 2.8) (drill 1.3) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.1) (tstamp ca89d809-1780-45d6-b08c-d42f04e70ca4))
  (pad "2" thru_hole circle (at 2.5 0) (size 2.8 2.8) (drill 1.3) (layers "*.Cu" "*.Mask") (tstamp 85bc6e82-f2f2-4c8c-9bf4-a49546e70068))
  (model "${KIPRJMOD}/../assets/3dmodels/1935161.stp"
    (offset (xyz -32.6 -44.65 -39))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 -90))
  )
)
