(footprint "Connector_Header_Vert_10POS" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -10.8 unlocked) (layer "F.SilkS")
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    (tstamp 42d28d18-b652-4faa-a8b1-567e84fe80b6)
  )
  (fp_text value "Connector_Header_Vert_10POS" (at 0 6.8 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 6f1a2b34-f753-4000-b870-c9ccf50f630e)
  )
  (fp_text user "${REFERENCE}" (at 0 0.05 -90) (layer "F.Fab")
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    (tstamp 36057df7-eadf-4647-b3e3-3107feebfa97)
  )
  (fp_rect (start -4.5 -10.18) (end 4.5 10.18)
    (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp 0825aad1-9ff9-46f8-b21d-b1727cd1bc6d))
  (fp_rect (start -4.5 -2.25) (end -3.3 2.25)
    (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp ae22b7f8-6c6f-4c57-b6e0-b291c86bbbcf))
  (fp_circle (center -3.7 -9.4) (end -3.252786 -9.4)
    (stroke (width 0.12) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 7f3cc88d-4d2e-4caf-b11f-93f5a0cb6adb))
  (fp_poly
    (pts
      (xy -3.7 -5.08)
      (xy -4.5 -4.53)
      (xy -4.5 -5.63)
    )

    (stroke (width 0.12) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 33db14e0-0354-4129-b679-24761df07dda))
  (fp_rect (start -4.6 -10.3) (end 4.6 10.3)
    (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp 2726e3af-44e8-4887-bf12-793186746ac7))
  (fp_rect (start -4.5 -10.18) (end 4.5 10.18)
    (stroke (width 0.12) (type solid)) (fill none) (layer "F.Fab") (tstamp 1da51e61-27c4-40d0-92d3-d02b3178981d))
  (fp_rect (start -4.5 -2.25) (end -3.3 2.25)
    (stroke (width 0.12) (type default)) (fill none) (layer "F.Fab") (tstamp f064d4c9-ded7-4af0-8f1c-b1ab4d94e7fd))
  (fp_rect (start -3.17 -9.2) (end 3.17 9.2)
    (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp f3b74d30-10c6-4ac4-be28-995b808fb02a))
  (pad "1" thru_hole circle (at -1.27 -5.08) (size 1.5 1.5) (drill 1.2) (layers "*.Cu" "*.Mask") (tstamp f59e8a60-1520-4e09-bf1e-0669ee5a08e4))
  (pad "2" thru_hole circle (at 1.27 -5.08) (size 1.5 1.5) (drill 1.2) (layers "*.Cu" "*.Mask") (tstamp 2e2f883b-9fdf-4219-8fa3-03165bbf58c8))
  (pad "3" thru_hole circle (at -1.27 -2.54) (size 1.5 1.5) (drill 1.2) (layers "*.Cu" "*.Mask") (tstamp 02681c2d-d0c0-44ef-8dcc-547d1da8f828))
  (pad "4" thru_hole circle (at 1.27 -2.54) (size 1.5 1.5) (drill 1.2) (layers "*.Cu" "*.Mask") (tstamp 75be8b15-9d8a-4e52-b1fb-c6bb82716214))
  (pad "5" thru_hole circle (at -1.27 0) (size 1.5 1.5) (drill 1.2) (layers "*.Cu" "*.Mask") (tstamp f8429703-c00e-4a94-957d-4bae14ef14e1))
  (pad "6" thru_hole circle (at 1.27 0) (size 1.5 1.5) (drill 1.2) (layers "*.Cu" "*.Mask") (tstamp 9b0591cd-c55a-4b40-a22a-fcb927ea343c))
  (pad "7" thru_hole circle (at -1.27 2.54) (size 1.5 1.5) (drill 1.2) (layers "*.Cu" "*.Mask") (tstamp e7c4ca31-47db-4b6c-8705-d29b604a3cc8))
  (pad "8" thru_hole circle (at 1.27 2.54) (size 1.5 1.5) (drill 1.2) (layers "*.Cu" "*.Mask") (tstamp fb053960-0ef4-4a0e-9b51-7c1fb6e085e5))
  (pad "9" thru_hole circle (at -1.27 5.08) (size 1.5 1.5) (drill 1.2) (layers "*.Cu" "*.Mask") (tstamp 383cb4b8-7019-4739-b48c-280ea556f64c))
  (pad "10" thru_hole circle (at 1.27 5.08) (size 1.5 1.5) (drill 1.2) (layers "*.Cu" "*.Mask") (tstamp 1332e057-a209-487f-b07b-aecd9a49a080))
  (model "${KIPRJMOD}/../assets/3dmodels/61201021621.stp"
    (offset (xyz -1.28 5.1 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 90))
  )
)
