(footprint "TerminalBlock_PhoenixContact_5x5mm" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -5.6 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 05d741ae-aaf0-47b1-a8c9-12f1cda327e6)
  )
  (fp_text value "TerminalBlock_PhoenixContact_5x5mm" (at 0 5.5 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 28047212-b786-4e24-9c6d-d27d6090dc73)
  )
  (fp_text user "${REFERENCE}" (at 0 7 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 57460716-14d5-4f8c-807d-af9089a852af)
  )
  (fp_line (start -11.8 -1) (end -11.8 1)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7cffc258-71a6-4556-afd2-c8b0f46b76db))
  (fp_line (start -11 -1.8) (end -9 -1.8)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2e4d6607-a720-4d14-a698-e08ff2390612))
  (fp_line (start -11 1.8) (end -9 1.8)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 96a6aaa0-8561-41e4-9021-839b8e7ed6e1))
  (fp_line (start -8.2 -1) (end -8.2 1)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 816d52b0-18dc-4e86-9efd-413906fc03e2))
  (fp_rect (start -12.5 -4.15) (end 12.5 -3.65)
    (stroke (width 0.12) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 091d4a37-4073-483e-ab12-27d50bb34999))
  (fp_rect (start -12.5 -4.15) (end 12.5 4.15)
    (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp 79feb21a-a935-421c-aa86-75cba8fa48cb))
  (fp_arc (start -11.8 -1) (mid -11.565685 -1.565685) (end -11 -1.8)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8db0cba3-b453-4c02-9fda-d44774de15da))
  (fp_arc (start -11 1.8) (mid -11.565685 1.565685) (end -11.8 1)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5d7146f3-1992-4b4d-8ed2-ef060d3cf87a))
  (fp_arc (start -9 -1.8) (mid -8.434315 -1.565685) (end -8.2 -1)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e92d9541-c757-4c13-8e75-9d0a10624122))
  (fp_arc (start -8.2 1) (mid -8.434315 1.565685) (end -9 1.8)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d6ac3042-0669-4531-a677-7a2a06ef6337))
  (fp_circle (center -5 0) (end -3.6 1.2)
    (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp 4226e09f-e7fc-4e63-a823-f4872af1a177))
  (fp_circle (center 0 0) (end 1.4 1.2)
    (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp c0fbd3e6-3d1a-436c-bf01-6ecf4a870f6d))
  (fp_circle (center 5 0) (end 6.4 1.2)
    (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp 712113ad-70c6-4737-8b1e-ebe3eb167681))
  (fp_circle (center 10 0) (end 11.4 1.2)
    (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp 5f83407e-0e19-4f00-a3cf-0e7b009a7958))
  (fp_poly
    (pts
      (xy -9.103852 4.136426)
      (xy -10.953852 4.136426)
      (xy -10.003852 2.586426)
    )

    (stroke (width 0.12) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 40bbdafa-0d2a-4c92-8249-e2b7b9679ef6))
  (fp_poly
    (pts
      (xy -4.1135 4.13786)
      (xy -5.9635 4.13786)
      (xy -5.0135 2.58786)
    )

    (stroke (width 0.12) (type solid)) (fill solid) (layer "F.SilkS") (tstamp c7170e2e-3cb3-45a6-a96f-0d5d4d12ee14))
  (fp_poly
    (pts
      (xy 0.8865 4.13786)
      (xy -0.9635 4.13786)
      (xy -0.0135 2.58786)
    )

    (stroke (width 0.12) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 40b22fe9-3116-45c1-80d5-55d38d670cf5))
  (fp_poly
    (pts
      (xy 5.8865 4.13786)
      (xy 4.0365 4.13786)
      (xy 4.9865 2.58786)
    )

    (stroke (width 0.12) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 31566e72-7193-4c16-afbb-270b7a268b6c))
  (fp_poly
    (pts
      (xy 10.8865 4.13786)
      (xy 9.0365 4.13786)
      (xy 9.9865 2.58786)
    )

    (stroke (width 0.12) (type solid)) (fill solid) (layer "F.SilkS") (tstamp d742d9b7-8d52-4a2d-a04f-034102ba07f2))
  (fp_rect (start -13 -4.5) (end 12.9 4.5)
    (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp ba1e98cc-4582-450b-8e8e-2bf0fdf0562a))
  (fp_rect (start -12.5 -4.15) (end 12.5 4.15)
    (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 416879e5-e0e5-484e-8891-a756da849ad5))
  (fp_rect (start -10.95 4.15) (end -9.05 2.45)
    (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 44af749e-6982-47aa-9da5-efb9b7fe7eff))
  (fp_rect (start -10.5 -0.45) (end -9.5 0.55)
    (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 4ee19190-51c4-43a6-8526-e9a182ef9b18))
  (fp_rect (start -6 2.45) (end -4.1 4.15)
    (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 123ef335-18af-401d-bf18-a389e3cbd034))
  (fp_rect (start -5.5 -0.45) (end -4.5 0.55)
    (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp b50d3ca7-1cfb-4e54-848c-ed75f3597a12))
  (fp_rect (start -1 2.45) (end 0.9 4.15)
    (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 5d472e77-0b87-4b54-bf34-5b3acfdc2c04))
  (fp_rect (start -0.5 -0.45) (end 0.5 0.55)
    (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 9d618276-1da7-4120-8da5-44c9ef46abbd))
  (fp_rect (start 4 2.45) (end 5.9 4.15)
    (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 36d31d0b-55f1-4d7f-9eda-8962f5fc153c))
  (fp_rect (start 4.5 -0.45) (end 5.5 0.55)
    (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 7475f940-1461-4ff0-914c-4d636d877b50))
  (fp_rect (start 9 2.45) (end 10.9 4.15)
    (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp cc38e3cc-b7ef-41da-a6c6-6471d6ca3ec5))
  (fp_rect (start 9.5 -0.45) (end 10.5 0.55)
    (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 77c5060e-6ba0-417a-9d5f-6b9fc02dcecb))
  (pad "1" thru_hole roundrect (at -10 0) (size 2.8 2.8) (drill 1.3) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.1) (tstamp 65527e2e-0a24-4526-811f-8f9f36f7f3ab))
  (pad "2" thru_hole circle (at -5 0) (size 2.8 2.8) (drill 1.3) (layers "*.Cu" "*.Mask") (tstamp 237f0411-0fc4-4e9e-8270-9a2223dd8568))
  (pad "3" thru_hole circle (at 0 0) (size 2.8 2.8) (drill 1.3) (layers "*.Cu" "*.Mask") (tstamp 5304cf30-937a-42cf-9239-026de4da32b5))
  (pad "4" thru_hole circle (at 5 0) (size 2.8 2.8) (drill 1.3) (layers "*.Cu" "*.Mask") (tstamp 292504f4-06dc-4be7-87a2-eccf5270365c))
  (pad "5" thru_hole circle (at 10 0) (size 2.8 2.8) (drill 1.3) (layers "*.Cu" "*.Mask") (tstamp bd9ac403-682c-4d5c-8188-dbfaf423a8d8))
  (model "${KIPRJMOD}/../assets/3dmodels/1935190.stp"
    (offset (xyz -12.5 -4.25 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
